
**Category 6 Shielded Keystone Jack**



Category 6 shielded keystone jack is designed for superior performance and easy assembly, meets and exceeds ANSI/TIA-568.2-D and ISO/IEC 11801 2nd edition Category 6 standards, supporting Gigabit Ethernet application and beyond. Narrow width design fits 24 ports in one unit panel for most efficient use of 1U panel.

## **Features**

Zinc-alloy metal shell

Contacts are phosphor bronze plated with 50 micro inches hard gold

Dual T568A &amp; T568B wiring

Polycarbonate 94V0 rated

Itertek ETL / Force EC Cat.6A VERIFIED

4PPoE compliant in accordance with IEEE802.bt Type 4

**Ordering Information**

|  |  |
| --- | --- |
| **Part No.** | **Description** |
| **1A68TPZ00** | RJ45, 8-Conductor Cat.6, Tool-free, Shielded, 180 degree, H.D. version |
| **2A68KPS00** | RJ45, 8-Conductor Cat.6, KRONE/110 IDC, Shielded, 180 degree, H.D. version |
| **5A68TPZ00** | RJ45, 8-Conductor Cat.6, Tool-free, Shielded, 180 degree, H.D. version |
| **6A68TPZ00** | RJ45, 8-Conductor Cat.6, Tool-free, Shielded, 180 degree, H.D. version |
| **7A68TPZ00** | RJ45, 8-Conductor Cat.6, Tool-free, Shielded, 180 degree, H.D. version |
| **1B68TPZ00** | RJ45, 8-Conductor Cat.6, Tool-free, Shielded, 180 degree, H.D. version, fits 0.5U panel |
| **7B68TPZ00** | RJ45, 8-Conductor Cat.6, Tool-free, Shielded, 180 degree, H.D. version, fits 0.5U panel |
| **1K68KPS00** | RJ45, 8-Conductor Cat.6, KRONE/110 IDC, Shielded, 90 degree, H.D. version |
| **2K68TPZ00** | RJ45, 8-Conductor Cat.6, KRONE/110 IDC, Shielded, 90 degree, Short depth design, L=29.86mm |
| **0T68TPZ00** | RJ45, 8-Conductor Cat.6, Tool-free, Shielded, 90 degree, H.D. version |
| **1T68TPZ00** | RJ45, 8-Conductor Cat.6, Tool-free, Shielded, 90 degree, H.D. version, L=34.5mm |