
Category 6 Shielded Keystone Jack



Category 6 shielded keystone jack is designed for superior performance and easy assembly, meets and exceeds ANSI/TIA-568.2-D and ISO/IEC 11801 2nd edition Category 6 standards, supporting Gigabit Ethernet application and beyond. Narrow width design fits 24 ports in one unit panel for most efficient use of 1U panel.

Features

Zinc-alloy metal shell

Contacts are phosphor bronze plated with 50 micro inches hard gold

Dual T568A &amp; T568B wiring

Polycarbonate 94V0 rated

Itertek ETL / Force EC Cat.6A VERIFIED

4PPoE compliant in accordance with IEEE802.bt Type 4

Ordering Information

|  |  |
| --- | --- |
| PART | Description |
| 1A68TPZ00 | RJ45, 8-Conductor Cat.6, Tool-free, Shielded, 180 degree, H.D. version |
| 2A68KPS00 | RJ45, 8-Conductor Cat.6, KRONE/110 IDC, Shielded, 180 degree, H.D. version |
| 5A68TPZ00 | RJ45, 8-Conductor Cat.6, Tool-free, Shielded, 180 degree, H.D. version |
| 6A68TPZ00 | RJ45, 8-Conductor Cat.6, Tool-free, Shielded, 180 degree, H.D. version |
| 7A68TPZ00 | RJ45, 8-Conductor Cat.6, Tool-free, Shielded, 180 degree, H.D. version |
| 1B68TPZ00 | RJ45, 8-Conductor Cat.6, Tool-free, Shielded, 180 degree, H.D. version, fits 0.5U panel |
| 7B68TPZ00 | RJ45, 8-Conductor Cat.6, Tool-free, Shielded, 180 degree, H.D. version, fits 0.5U panel |
| 1K68KPS00 | RJ45, 8-Conductor Cat.6, KRONE/110 IDC, Shielded, 90 degree, H.D. version |
| 2K68TPZ00 | RJ45, 8-Conductor Cat.6, KRONE/110 IDC, Shielded, 90 degree, Short depth design, L=29.86mm |
| 0T68TPZ00 | RJ45, 8-Conductor Cat.6, Tool-free, Shielded, 90 degree, H.D. version |
| 1T68TPZ00 | RJ45, 8-Conductor Cat.6, Tool-free, Shielded, 90 degree, H.D. version, L=34.5mm |